**(A). SCHEDULE OF MATERIALS FOR YOUR PROPOSED GROUND FLOOR BLOCKWORK & SEPTIC TANK CONSTRUCTION.**

**CLIENT: MR. SULAIMAN ALAKETU**

**LOCATION: GBERIGBE-IKORODU, LAGOS STATE.**

**1. BLOCKWORK (282sq.m)**

**(i) 9" Block-2500nos**

**(ii) Sharp Sand- 30tons**

**(iii) Cement- 50bags**

**2. CONCRETEWORK (1:3:4)—11.18cu.m**

**(i) Cement: 55bags**

**(ii) Sharp Sand: 10tons**

**(iii) Granite: 15tons**

**(3) REINFORCEMENT BAR:**

**(i) 16mm bar: 29Lengths**

**(ii) 12mm bar: 40Lengths**

**(iii)10mm bar: 36Lengths**

**(iv) Binding wire: 20kg**

**(4) FORMWORK**

**(i) 1\*12 plank: 80nos**

**(ii) 2\*3 plank: 30nos**

**(iii) 3” Nail: 1bag of 3” nails**

**(B). SCHEDULE OF LABOUR FOR YOUR PROPOSED FIRST FLOOR BLOCKWORK & SEPTIC TANK CONSTRUCTION.**

**CLIENT: MR. SULAIMAN ALAKETU**

**LOCATION: GBERIGBE-IKORODU, LAGOS STATE.**

**(1) BLOCKWORK: 282sq.m @ #800/sq.m-----#225,600**

**(2) CONCRETEWORK: 11.18cu.m @#8,000/cu.m.**

**--------------#89,440**

**(3) REINFORCEMENT BAR:**

**1.26tonnes @ #60,000/tonnes ----------#75,600**

**(4) FORMWORK:**

**103.11sq.m @ #800/sq.m-------#82,488.**

**SUB-TOTAL-------------#473,128.**

**Regards,**

**Idrees Abdulquadri**

**Project Engineer.**